**Floor with 8mm entrance**

National 460mm

Langstroth 508mm

**C**

**F**

8mm gap

5mm groove cut into side pieces for wire mesh

**E**

**D**

**A**

44mm

44mm

18m

18mm

94mm

**B**

15 Degree Angle angle

**Material List** NATIONAL LANGSTROTH

A 2 x 18mm thick x 94mm deep x 460mm long 2 x 18mm thick x 94mm Deep x 508mm Long

B 1 x 44mm thick x 44mm deep x 424mm long 1 x 44mm thick x 44mm deep x 380mm long

C 1 x 18mm thick x 18mm deep x 424mm long 1 x 18mm thick x 18mm deep x 380mm long

D 1 x 18mm thick x 70mm deep x 424mm long 1 x 18mm thick x 70mm deep x 380mm long

E 1 x 18mm thick x 94mm deep x 424mm long 1 x 18mm thick x 94mm deep x 424mm long

F 1 x mesh flooring cut to 434mm wide x 408mm long 1 x mesh flooring cut to 390mm wide x 456mm long